**Digital talking watch**

*Note:* Hold **MODE** and **TALKING** button for 3 seconds to enter power-saving mode.

**FEATURES:**

**Time and Date Announcement** – Watch tells the time as well as the date

**Four Talking Alarms** – Helps to remind you of daily routines eg: medicine taking times.

**Talking Stopwatch with Lap** – Lets you keep track of your time spent on activities and record lap times.

**Hourly Time Announcement** – Automatically tells the time every hour on the hour.



**Orientation:**

Position the watch in front of you. You will notice the following buttons:

**Talk button** - Top right hand side (2 o’clock)

**Set button** – Bottom right hand side (4 o’clock) (This button also speaks the date)

**Adjust button** – Bottom left hand side (8 o’clock)

**Mode button** - Top left hand side (10 o’clock)

**SETTING THE TIME, 12H/24H, YEAR, MONTH AND DATE:**

Note: While setting the time and date, if you do not press any key for 1 minute, the watch will confirm and return to the current time display.

**Follow these steps to set the date and time.**

1. Repeatedly press **MODE** until you hear the time announcement and the display shows the time and day of the week.
2. Press and hold down **SET** for more than 2 seconds until you hear “Time set” and the 12H or 24H digits flash on the display.
3. Repeatedly press **ADJ** to select 12H or 24H. The watch announces “12” or “24” and flashes the digits on the display.
4. Press **SET**, you hear “hour set” and the hour digits flash.
5. Repeatedly press (or hold down) **ADJ** to set the correct hour. The watch announces the hour as it advances on the display.
6. Press **SET**, you hear “Minute set” and the minute digits flash.
7. Repeatedly press (or hold down) **ADJ** to set the correct minute. The watch announces the minute as it advances on the display.
8. Press **SET**, you hear “Year set” and the year digits flash.
9. Repeatedly press (or hold down) **ADJ** to set the correct year. The watch announces the year as it advances on the display.
10. Press **SET**, you hear “Month set” and the month digits flash.
11. Repeatedly press (or hold down) **ADJ** to set the correct month. The watch announces the month as it advances on the display.
12. Press **SET**, you hear “Day set” and the day digits flash.
13. Repeatedly press (or hold down) **ADJ** to set the correct day. The watch announces the day as it advances on the display.
14. Press **MODE** to complete setting and return to the time display.

**LISTENING TO THE TIME AND DATE ANNOUNCEMENTS**

To hear the time announcement, simply press **TALKING**. The watch announces the time eg: “It is 10.25AM”

To hear the date announcement press **SET**, the watch announces the day eg: “Today is the twenty-third” (the month is not announced). Press **SET** again and it will display the year, press **SET** again and it will return to the normal time display.

**SETTING THE ALARM**

Note: The watch lets you set 4 daily alarms. While setting the alarm time, if you do not press any key for more than 1 minute the watch will confirm and return to the Alarm time display.

Follow these steps to set the alarm.

1. Repeatedly press **MODE** until you hear “Alarm One” and AL and -1 appear on the LCD.
2. Press and hold down **SET** for more than 2 seconds until you hear “Alarm 1 set, hour set: and the hour digits flash on the display.
3. Repeatedly press (or hold down) **ADJ** to set the hour. The watch announces the hour as it advances on the display.
4. Press **SET**, you hear “Minute set” and the minute digits flash.
5. Repeatedly press (or hold down) **ADJ** to set the correct minute. The watch announces the minute as it advances on the display.
6. Press **MODE** to complete Alarm 1 time setting.
7. Repeatedly press **ADJ** until you hear “Alarm 1 on” and a bell symbol appears on the display to turn on the alarm.
8. Repeat steps 1 to 7 to set alarm 2, 3 and 4.
9. Repeatedly press **MODE** until you hear the current time announcement to return to the time display.

**TURNING THE ALARM ON AND OFF**

You can easily turn on and turn off the alarm using the following steps.

1. Repeatedly press **MODE** until you hear “Alarm one”
2. To turn on the alarm, repeatedly press **ADJ** until you hear “Alarm one on” and a bell symbol appears on the display. To turn off the alarm, press **ADJ** again and you hear “Alarm one off” and the bell symbol disappears.
3. Press **MODE** to go to Alarm 2 and repeatedly press **ADJ** to turn on/off alarm 2.
4. Repeat step 3 for alarm 3 and 4.

At the pre-set alarm time, the alarm sounds for 1 minute and turns off automatically. To silence the alarm sooner, press any key. The following is an example of the alarm sound “Alarm 2, Good morning, it is 7.30AM, di, di, di, di” repeating for one minute.

**TURNING THE HOURLY TIME ANNOUNCEMENT ON OR OFF**

You can set the watch to announce the time every hour on the hour. To turn on the hourly report, repeatedly press **ADJ** until you hear “Hourly report on” and symbol with a small dot and three curved lines on either side appears on the display. To turn off the hourly report, press **ADJ** again and your hear “Hourly report off” and the symbol disappears.

**USING THE STOPWATCH (COUNT UP TIMER)**

The maximum count up timer (stopwatch) is 24 hours. When the timer reaches 23:59:59, it resets to 0:00:00 and begins counting up again.

Follow these steps to operate the stopwatch.

1. Repeatedly press **MODE** until you hear “Stopwatch” and “ST” appears on the display.
2. If the display does not show 0:00:00, following these steps to reset to 0:00:00.

Case 1: When the time is not running (digits do not change, and “:” is not flashing) press **SET** once then”0:00:00” will appear on the display.

Case2: When the timer is running in the front (digits are changing) Press **ADJ** then **SET** to reset to 0:00:00.

Case 3: When the timer is running in the background (digits do not change and “:” is flashing) press **ADJ** then **SET** twice to reset to 0:00:00.

1. Press ADJ to start the timer. The stopwatch starts and announces timing.
2. To stop or pause count up press **ADJ**. To resume the timer, press **ADJ** again and the stopwatch timer continues from the displayed time.
3. To reset the timer to 0:00:00 press **ADJ** to stop the timer and then press **SET**.

**RECORDING LAP TIMES**

The lap function lets you freeze the display, document the times reading and then return to the stopwatch timer to see the advancing time. You can monitor lap times continuously as long as the stopwatch continues to run.

Follow these steps to measure lap times.

1. Repeatedly press **MODE** until you hear “Stopwatch” and “ST” appears on the display.

Note: If the display does not show):00:00, follow the steps described in **USING STOPWATCH** to reset to 0:00:00.

1. Press **ADJ** to start the stopwatch timer
2. When the first lap is finished, press **SET**. The stopwatch display freezes, but the stopwatch timer continues to run in the background. The “:” in the elapsed time flashes to show that it is running in the background.
3. When you have documented the lap time, press **SET**. The display changed to show the advancing time (that was previously continuing in the background) on the stopwatch timer.
4. Repeat steps 3 and 4 for each additional lap.
5. Press **ADJ** to stop the stopwatch. Then press **SET** to reset the display to 0:00:00.

The stop watch announces the elapsed time according to the following:

**Elapsed time** **Voice announcement**

0 to 9 seconds every second

10 to 59 seconds every 10 seconds

1 to 9 minutes every minute

Over 10 minutes every 10 minutes

During timing you can press **TALKING** to hear the voice announcement at any time.

**WARRANTY INFORMATION:**

The Blind Foundation grants a warranty of 1 year from the date of purchase, this covers repairs or replacement in the event of defects in materials or workmanship. In such cases, the defective product will be repaired or replaced as determined by The Blind Foundation. This warranty does not cover damages caused by accident, improper use or unauthorized modifications. In addition, this warranty does not cover expendable materials and defects which constitute normal wear and tear. Please contact The Blind Foundation on

0800 24 33 33 for warranty questions or service.

# How to contact the Blind Foundation

Phone number: 0800 24 33 33

Postal address: Blind Foundation, Awhina House, 4 Maunsell Road, Parnell, Auckland 1052

Email: generalenquiries@blindfoundation,org.nz

Web address: www.blindfoundation.org.nz